# ---------------------------------------------------------------------------------------------------
# Scenario simulation 
# ---------------------------------------------------------------------------------------------------
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 1000 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 12.81305185953776
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-1000.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x62f95585ddb0
0x62f95585db70
0x62f95594ed40
0x62f95594ec60
0x62f95594eba0
0x62f95594e530
0x62f9558f4cd0
0x62f9558d32a0
0x62f9554834a0
0x62f955867710
0x62f9558e2df0
0x62f955868910
rain total: 12.8131
runoff total: 8.85362
infil total: 3.95944
start fastflood function 0x7ebf6191c010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x62f955483c90
 i 10x62f95594e120
 i 20x62f9558e2c20
 i 30x62f9558671b0
 i 40x62f955862b60
 i 50x62f95586c100
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Maximum observed q: 7722
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-1000.csv
duration: 1.30126 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 500 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 11.834416707356771
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-500.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x64401125ed30
0x64401125eaf0
0x64401125ddd0
0x64401125dcf0
0x64401125dc10
0x64401134f520
0x6440112f5cd0
0x6440112d42a0
0x644010e86780
0x64401134b160
0x6440112e3df0
0x64401134af70
rain total: 11.8344
runoff total: 7.89089
infil total: 3.94352
start fastflood function 0x7d988719e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x64401134eeb0
 i 10x644010e885a0
 i 20x644011265630
 i 30x644011261880
 i 40x644011266a30
 i 50x644011267270
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 6857
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-500.csv
duration: 0.957159 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 200 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 10.577882766723633
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-200.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5855b2789fc0
0x5855b2789d80
0x5855b279e080
0x5855b279dfa0
0x5855b279dec0
0x5855b287b510
0x5855b2821cc0
0x5855b2800290
0x5855b23b2260
0x5855b280fde0
0x5855b27932e0
0x5855b287b170
rain total: 10.5779
runoff total: 6.66687
infil total: 3.91101
start fastflood function 0x7e9d226a2010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5855b23b0bd0
 i 10x5855b2810f60
 i 20x5855b23b0480
 i 30x5855b287d6e0
 i 40x5855b23b3950
 i 50x5855b23b4190
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 5756
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-200.csv
duration: 0.935114 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 100 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 9.648907979329428
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-100.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5a3c6e179fc0
0x5a3c6e179d80
0x5a3c6e18e060
0x5a3c6e18df80
0x5a3c6e18dec0
0x5a3c6e26b520
0x5a3c6e211cc0
0x5a3c6e1f0290
0x5a3c6e18de00
0x5a3c6dda3d90
0x5a3c6dda0450
0x5a3c6e1797f0
rain total: 9.64891
runoff total: 5.77476
infil total: 3.87414
start fastflood function 0x7c4631a50010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5a3c6e14d960
 i 10x5a3c6e1852f0
 i 20x5a3c6e1501a0
 i 30x5a3c6e189580
 i 40x5a3c6dda1710
 i 50x5a3c6e266390
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 4961
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-100.csv
duration: 0.951326 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 50 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 8.732931772867838
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-50.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x6468eaab7db0
0x6468eaab7b70
0x6468eaba8d40
0x6468eaba8c60
0x6468eaba8ba0
0x6468eaba8530
0x6468eab4ecd0
0x6468eab2d2a0
0x6468eaacb0d0
0x6468eaac5980
0x6468eaacae70
0x6468eaac8b80
rain total: 8.73293
runoff total: 4.90977
infil total: 3.82316
start fastflood function 0x7b7ab1b9e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x6468eaa84f40
 i 10x6468eaba83d0
 i 20x6468eab2d2a0
 i 30x6468eab3a500
 i 40x6468eaabae40
 i 50x6468eaba2de0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 4222
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-50.csv
duration: 0.946094 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 40 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 8.406804402669271
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-40.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x58254771ffc0
0x58254771fd80
0x582547734060
0x582547733f80
0x582547733ec0
0x582547811520
0x5825477b7cc0
0x582547796290
0x5825476f38a0
0x582547346450
0x5825477a5de0
0x58254780c870
rain total: 8.4068
runoff total: 4.60615
infil total: 3.80065
start fastflood function 0x786385f9e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x58254772a0d0
 i 10x5825476f5f60
 i 20x582547796290
 i 30x582547733510
 i 40x582547729170
 i 50x58254771f100
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 3961
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-40.csv
duration: 0.95733 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 20 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 7.533549626668294
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-20.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5aea3237cfc0
0x5aea3237cd80
0x5aea32391080
0x5aea32390fa0
0x5aea32390ec0
0x5aea3246e4f0
0x5aea32414cc0
0x5aea323f3290
0x5aea31fa7b10
0x5aea31fa3450
0x5aea3237ce40
0x5aea32402de0
rain total: 7.53355
runoff total: 3.80711
infil total: 3.72644
start fastflood function 0x70de0039e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5aea31fa5a20
 i 10x5aea31fa7b50
 i 20x5aea31fa5f10
 i 30x5aea32470090
 i 40x5aea3246d6e0
 i 50x5aea31fa6b90
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 3266
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-20.csv
duration: 0.951385 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 10 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 6.628482182820638
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-10.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x649e42effd10
0x649e42effad0
0x649e42efedb0
0x649e42efecd0
0x649e42efec10
0x649e42ff0550
0x649e42f96cd0
0x649e42f07240
0x649e42feb930
0x649e42f752a0
0x649e42fec160
0x649e42f84df0
rain total: 6.62848
runoff total: 3.00245
infil total: 3.62603
start fastflood function 0x7cfde3c7a010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x649e42b22fb0
 i 10x649e42f85d30
 i 20x649e42ed5120
 i 30x649e42f82500
 i 40x649e42f0db60
 i 50x649e42f0e3a0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 2560
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-10.csv
duration: 0.947811 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 5 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 5.719692230224609
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-5.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x60cdf26f7fd0
0x60cdf26f7d90
0x60cdf270c090
0x60cdf270bfb0
0x60cdf270bed0
0x60cdf27e9500
0x60cdf278fcd0
0x60cdf276e2a0
0x60cdf2320260
0x60cdf2322590
0x60cdf2703d70
0x60cdf27e9780
rain total: 5.71969
runoff total: 2.22253
infil total: 3.49717
start fastflood function 0x79f07179e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x60cdf2701ff0
 i 10x60cdf26cdeb0
 i 20x60cdf2700370
 i 30x60cdf277b830
 i 40x60cdf26f8840
 i 50x60cdf2700760
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 1876
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-5.csv
duration: 0.957207 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: Current | Climate: Historic | TR: 2 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif
Check arg -rain
Set arg rain
Arg value 4.5037078857421875
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-2.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x61d888eb3db0
0x61d888eb3b70
0x61d888fa4d50
0x61d888fa4c70
0x61d888fa4b90
0x61d888fa4520
0x61d888f4acd0
0x61d888f292a0
0x61d888eb9d50
0x61d888fa47a0
0x61d888ec1dd0
0x61d888ec3cc0
rain total: 4.50371
runoff total: 1.24861
infil total: 3.2551
start fastflood function 0x7ef347021010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x61d888eb7e50
 i 10x61d888ebcd60
 i 20x61d888ebb4a0
 i 30x61d888f36500
 i 40x61d888fa2cd0
 i 50x61d888fa3510
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 1032
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_Current_TR-2.csv
duration: 0.932555 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 1000 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 12.81305185953776
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-1000.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x62bf5a6490b0
0x62bf5a648e70
0x62bf5a647910
0x62bf5a73a250
0x62bf5a73a170
0x62bf5a739c10
0x62bf5a6d5030
0x62bf5a654e90
0x62bf5a6479d0
0x62bf5a647f70
0x62bf5a657e10
0x62bf5a650390
rain total: 12.8131
runoff total: 9.01722
infil total: 3.79583
start fastflood function 0x75bf03493010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x62bf5a6571f0
 i 10x62bf5a6c9e80
 i 20x62bf5a61deb0
 i 30x62bf5a65ae30
 i 40x62bf5a738310
 i 50x62bf5a6bd210
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 8412
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-1000.csv
duration: 0.964756 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 500 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 11.834416707356771
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-500.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x59337af32040
0x59337af31e00
0x59337af310e0
0x59337af31000
0x59337af30f20
0x59337af309c0
0x59337afbe020
0x59337af44710
0x59337af415d0
0x59337afb6bd0
0x59337ab5b470
0x59337ab5b530
rain total: 11.8344
runoff total: 8.05334
infil total: 3.78108
start fastflood function 0x7a4434b9e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x59337ab5a450
 i 10x59337afb6ac0
 i 20x59337af43e80
 i 30x59337ab596b0
 i 40x59337ab5a6d0
 i 50x59337ab5af10
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 7600
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-500.csv
duration: 0.9641 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 200 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 10.577882766723633
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-200.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x64535ad66b70
0x64535ad66930
0x64535ae57dd0
0x64535ae57cf0
0x64535ae57c10
0x64535ad79c90
0x64535adf3030
0x64535ad78ac0
0x64535ae59b90
0x64535ade87d0
0x64535a98c0d0
0x64535ad665a0
rain total: 10.5779
runoff total: 6.8268
infil total: 3.75108
start fastflood function 0x7ab89929b010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x64535a989fb0
 i 10x64535ad66e70
 i 20x64535a98f950
 i 30x64535ae59b70
 i 40x64535ae56640
 i 50x64535addb210
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 6558
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-200.csv
duration: 0.951249 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 100 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 9.648907979329428
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-100.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x56554c8f7b60
0x56554c8f7920
0x56554c9e8dc0
0x56554c9e8ce0
0x56554c9e8c00
0x56554c90ac80
0x56554c984020
0x56554c979830
0x56554c8f7000
0x56554c51d160
0x56554c8f7800
0x56554c9e41d0
rain total: 9.64891
runoff total: 5.93179
infil total: 3.71712
start fastflood function 0x7ad46df69010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x56554c8d3110
 i 10x56554c8ccea0
 i 20x56554c9e41d0
 i 30x56554c8f8660
 i 40x56554c9e7630
 i 50x56554c8ff380
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 5789
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-100.csv
duration: 0.95297 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 50 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 8.732931772867838
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-50.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x58ac0946bb60
0x58ac0946b920
0x58ac0955cdc0
0x58ac0955cce0
0x58ac0955cc00
0x58ac0947ec80
0x58ac094f8020
0x58ac09475760
0x58ac09474060
0x58ac09094570
0x58ac0947b240
0x58ac0955ce80
rain total: 8.73293
runoff total: 5.0629
infil total: 3.67003
start fastflood function 0x7ab3b4f04010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x58ac094d4720
 i 10x58ac0947f010
 i 20x58ac09441020
 i 30x58ac094755c0
 i 40x58ac09479500
 i 50x58ac094e0140
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 5020
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-50.csv
duration: 0.947801 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 40 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 8.406804402669271
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-40.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x64601f690b70
0x64601f690930
0x64601f781dc0
0x64601f781ce0
0x64601f781c00
0x64601f6a3c90
0x64601f71d030
0x64601f2b8220
0x64601f2b9460
0x64601f690c30
0x64601f781940
0x64601f2b6160
rain total: 8.4068
runoff total: 4.75761
infil total: 3.6492
start fastflood function 0x7b541739c010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x64601f66c060
 i 10x64601f2b7ac0
 i 20x64601f2b7d80
 i 30x64601f68d280
 i 40x64601f69a460
 i 50x64601f780330
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 4745
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-40.csv
duration: 0.945376 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 20 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 7.533549626668294
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-20.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x58d5320d60a0
0x58d5320d5e60
0x58d5320d4900
0x58d5321c7220
0x58d5321c7140
0x58d5321c6c00
0x58d532162020
0x58d5320e1c00
0x58d5320e0260
0x58d5320d4b40
0x58d5320cd3a0
0x58d5321c6960
rain total: 7.53355
runoff total: 3.95314
infil total: 3.58041
start fastflood function 0x77f1086ec010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x58d531cf8fb0
 i 10x58d5320e0620
 i 20x58d5320aaf60
 i 30x58d531d3e230
 i 40x58d5320d43b0
 i 50x58d5321c5300
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 3998
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-20.csv
duration: 0.92897 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 10 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 6.628482182820638
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-10.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5aeb936500a0
0x5aeb9364fe60
0x5aeb9364e900
0x5aeb93741240
0x5aeb93741160
0x5aeb93740c00
0x5aeb936dc020
0x5aeb93657380
0x5aeb9364ef60
0x5aeb9365be80
0x5aeb9379f610
0x5aeb9364ff20
rain total: 6.62848
runoff total: 3.14134
infil total: 3.48715
start fastflood function 0x7a0d00d3c010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5aeb93275930
 i 10x5aeb93625020
 i 20x5aeb9365cef0
 i 30x5aeb9365ddf0
 i 40x5aeb9365b260
 i 50x5aeb9365baa0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 3206
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-10.csv
duration: 0.947159 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 5 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 5.719692230224609
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-5.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x57763f1cdf00
0x57763f1cdcc0
0x57763f1cc760
0x57763f2bf080
0x57763f2befa0
0x57763f2bea60
0x57763f259e80
0x57763f1d9a60
0x57763f1d80c0
0x57763f1cc9a0
0x57763f1c5200
0x57763f2be7c0
rain total: 5.71969
runoff total: 2.35172
infil total: 3.36798
start fastflood function 0x785005f9e010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x57763f1da7c0
 i 10x57763f1a90f0
 i 20x57763ee36110
 i 30x57763f24f180
 i 40x57763f1cbd90
 i 50x57763f1cc5d0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 2419
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-5.csv
duration: 0.941887 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: BaU | Climate: Historic | TR: 2 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif
Check arg -rain
Set arg rain
Arg value 4.5037078857421875
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-2.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_BaU.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_BaU.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x56ff101d4940
0x56ff101d4700
0x56ff101d39e0
0x56ff101d3900
0x56ff101d3820
0x56ff101e7ae0
0x56ff10260e80
0x56ff102c58e0
0x56ff101e7e20
0x56ff102c56b0
0x56ff101cc200
0x56ff1024a0d0
rain total: 4.50371
runoff total: 1.35592
infil total: 3.14779
start fastflood function 0x7c005043b010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x56ff0fdfaae0
 i 10x56ff10255cd0
 i 20x56ff101d4880
 i 30x56ff101e7880
 i 40x56ff102c4490
 i 50x56ff101e7940
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 1479
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_BaU_TR-2.csv
duration: 0.94593 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 1000 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 12.81305185953776
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-1000.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x59b6643b0b60
0x59b6643b0920
0x59b6644a1dc0
0x59b6644a1ce0
0x59b6644a1c00
0x59b6643c3c80
0x59b66443d020
0x59b663fd6160
0x59b6643c3ea0
0x59b6644a3b80
0x59b663fd8290
0x59b6643b09e0
rain total: 12.8131
runoff total: 9.00459
infil total: 3.80846
start fastflood function 0x701e9ccbf010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x59b66437de10
 i 10x59b663fd9910
 i 20x59b664435b90
 i 30x59b6644a3830
 i 40x59b6643b8320
 i 50x59b6643b8b60
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 8181
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-1000.csv
duration: 0.96246 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 500 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 11.834416707356771
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-500.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x64fe30176b70
0x64fe30176930
0x64fe30267dd0
0x64fe30267cf0
0x64fe30267c10
0x64fe30189c90
0x64fe30203030
0x64fe30180770
0x64fe3017f070
0x64fe30186250
0x64fe30267aa0
0x64fe30267e90
rain total: 11.8344
runoff total: 8.04072
infil total: 3.79369
start fastflood function 0x73a6010c9010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x64fe2fd9ec80
 i 10x64fe301fcca0
 i 20x64fe3017ed40
 i 30x64fe30184530
 i 40x64fe30266970
 i 50x64fe301eb750
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 7313
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-500.csv
duration: 0.949013 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 200 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 10.577882766723633
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-200.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x55fc59a630a0
0x55fc59a62e60
0x55fc59a61900
0x55fc59b54230
0x55fc59b54150
0x55fc59b53bf0
0x55fc59aef020
0x55fc59a5a3a0
0x55fc59b4f020
0x55fc59a62880
0x55fc59688160
0x55fc59ae4800
rain total: 10.5779
runoff total: 6.8142
infil total: 3.76368
start fastflood function 0x7ad358930010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x55fc59688930
 i 10x55fc59a6bf00
 i 20x55fc59a5f0c0
 i 30x55fc596cb200
 i 40x55fc59a69bf0
 i 50x55fc59a61a80
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 6200
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-200.csv
duration: 0.948608 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 100 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 9.648907979329428
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-100.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x56558c59fb60
0x56558c59f920
0x56558c690dc0
0x56558c690ce0
0x56558c690c00
0x56558c5b2c80
0x56558c62c020
0x56558c1c6b30
0x56558c1c8c70
0x56558c5973a0
0x56558c5a8080
0x56558c615270
rain total: 9.64891
runoff total: 5.91919
infil total: 3.72972
start fastflood function 0x7432e02c1010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x56558c1c7930
 i 10x56558c5a7d20
 i 20x56558c1bfe90
 i 30x56558c5afa30
 i 40x56558c1c3000
 i 50x56558c5a8d00
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 5382
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-100.csv
duration: 0.948787 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 50 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 8.732931772867838
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-50.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x599b75cf00a0
0x599b75cefe60
0x599b75cee900
0x599b75de1240
0x599b75de1160
0x599b75de0c00
0x599b75d7c020
0x599b75cf7380
0x599b75cee9c0
0x599b75cfbe80
0x599b75ceef60
0x599b75d65270
rain total: 8.73293
runoff total: 5.05035
infil total: 3.68258
start fastflood function 0x7b7adca2f010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x599b75915bd0
 i 10x599b75cfe7b0
 i 20x599b75cc5110
 i 30x599b75d00ab0
 i 40x599b75d75d50
 i 50x599b75cef700
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 4583
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-50.csv
duration: 0.942844 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 40 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 8.406804402669271
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-40.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x56d1222a2020
0x56d1222a1de0
0x56d1222a10c0
0x56d1222a0fe0
0x56d1222a0f00
0x56d1222a09c0
0x56d12232e020
0x56d12238dbc0
0x56d1222a2660
0x56d122326bd0
0x56d1222a24f0
0x56d1223f1610
rain total: 8.4068
runoff total: 4.7451
infil total: 3.66171
start fastflood function 0x7bcdbf83b010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x56d1222b3d90
 i 10x56d1222770e0
 i 20x56d12232f300
 i 30x56d1222b1b40
 i 40x56d1222aaeb0
 i 50x56d1222ab6f0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 4302
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-40.csv
duration: 0.942943 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 20 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 7.533549626668294
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-20.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5f2fa68b7b70
0x5f2fa68b7930
0x5f2fa69a8dd0
0x5f2fa69a8cf0
0x5f2fa69a8c10
0x5f2fa68cac90
0x5f2fa6944030
0x5f2fa68c9ac0
0x5f2fa69aab90
0x5f2fa69397d0
0x5f2fa64dd0d0
0x5f2fa68b75a0
rain total: 7.53355
runoff total: 3.94086
infil total: 3.59269
start fastflood function 0x7ef93bf8c010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5f2fa64dafb0
 i 10x5f2fa68b7e70
 i 20x5f2fa64e0950
 i 30x5f2fa69aab70
 i 40x5f2fa69a7640
 i 50x5f2fa692c210
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 3598
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-20.csv
duration: 0.933358 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 10 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 6.628482182820638
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-10.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x59d6191bab60
0x59d6191ba920
0x59d6192abdc0
0x59d6192abce0
0x59d6192abc00
0x59d6191cdc80
0x59d619247020
0x59d6191c4760
0x59d6191ca240
0x59d6192abe80
0x59d6192ac0c0
0x59d618de0160
rain total: 6.62848
runoff total: 3.12958
infil total: 3.4989
start fastflood function 0x70a243e7f010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x59d6191cdf50
 i 10x59d619240d50
 i 20x59d61923be70
 i 30x59d6191c9800
 i 40x59d6191c8a60
 i 50x59d6192aa0c0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 2887
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-10.csv
duration: 0.932969 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 5 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 5.719692230224609
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-5.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x62dca2bb9f10
0x62dca2bb9cd0
0x62dca2bb8770
0x62dca2cab090
0x62dca2caafb0
0x62dca2caaa70
0x62dca2bc5a70
0x62dca2c45e90
0x62dca2bc7280
0x62dca2caaef0
0x62dca2bc5cb0
0x62dca2c3b630
rain total: 5.71969
runoff total: 2.34091
infil total: 3.37878
start fastflood function 0x7b22e76c3010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x62dca2bc4250
 i 10x62dca2c3ae60
 i 20x62dca2c09360
 i 30x62dca2822140
 i 40x62dca2bb7eb0
 i 50x62dca2bbfea0
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 2191
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-5.csv
duration: 0.937826 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Execution FastFlood | Scenario: NbS | Climate: Historic | TR: 2 | Duration: 3.0 
# ---------------------------------------------------------------------------------------------------
[OUTPUT] FastFlood command line tool, version 0.3.5, May 20 2025
This version is intended for the use of WaterProof FastFlood project (C-N4W-100724)
This software is a commercial property of FastHazard, the Netherlands
Do not share this software without explicit permission of its original owner
 
Check arg /app/fastflood/fastflood
Check arg -customurl
Set arg customurl
Arg value https://dev.water-proof.org/wf-models/get-ff-data?dataset={d}&x={x}&y={y}&z={z}&date=&key=DGD3BHF78LNRX9A
Check arg -verbose
Set arg verbose
Check arg -sim
Set arg sim
Check arg -dem
Set arg dem
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif
Check arg -man
Set arg man
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif
Check arg -inf
Set arg inf
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif
Check arg -rain
Set arg rain
Arg value 4.5037078857421875
Check arg -dur
Set arg dur
Arg value 3.0
Check arg -whout
Set arg whout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Check arg -qout
Set arg qout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Check arg -vout
Set arg vout
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Check arg -hydrograph
Set arg hydrograph
Arg value /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-2.csv
Check arg -d_cal
Set arg d_cal
Number of threads: 1 8
Initializing GDAL
Done initializing gdal
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/DEM.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Manning_NbS.tif  Bandnr: 0
Read raster /app/outputs/fastflood/1000_34_2026-1-19/WI_15/in/06-FLOOD/Raster/Infiltration_NbS.tif  Bandnr: 0
Finished loading maps
Finished loading runfile
Domain reference map found (csx, csy, cols, rows):305.748  -305.748 283 354
Domain CRS: PROJCS["WGS 84 / Pseudo-Mercator",GEOGCS["WGS 84",DATUM["WGS_1984",SPHEROID["WGS 84",6378137,298.257223563,AUTHORITY["EPSG","7030"]],AUTHORITY["EPSG","6326"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","4326"]],PROJECTION["Mercator_1SP"],PARAMETER["central_meridian",0],PARAMETER["scale_factor",1],PARAMETER["false_easting",0],PARAMETER["false_northing",0],UNIT["metre",1,AUTHORITY["EPSG","9001"]],AXIS["Easting",EAST],AXIS["Northing",NORTH],EXTENSION["PROJ4","+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs"],AUTHORITY["EPSG","3857"]]
Model domain: width: 283 height: 354
duration: 3 hours 
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=11&z=0&date=&key=DGD3BHF78LNRX9A
Download url: https://dev.water-proof.org/wf-models/get-ff-data?dataset=PRECALIB&x=6&y=12&z=0&date=&key=DGD3BHF78LNRX9A
HTTP transfer completed with status 0
HTTP transfer completed with status 0
GlobalTile Data Size: 10 7
RangeD: -63.909 -63.1317 -18.4578 -17.5331
other: 0.1 0.1 
Range: 1160 1170 1076 1083
0x5faaf8d17f10
0x5faaf8d17cd0
0x5faaf8d16770
0x5faaf8e090b0
0x5faaf8e08fd0
0x5faaf8e08a70
0x5faaf8da3e90
0x5faaf8d23cf0
0x5faaf8e674e0
0x5faaf8d24670
0x5faaf8d16dd0
0x5faaf8d1f1f0
rain total: 4.50371
runoff total: 1.34753
infil total: 3.15618
start fastflood function 0x72e692765010 283 354 305.748 1
output wh with channel
piters: 0
in_fluxiters 120
start fastflood DEM correction 0.001 120
do q calc 120
workers done
0 cascade : 283 354
1 cascade : 95 118
2 cascade : 32 40
3 cascade : 11 14
4 cascade : 4 5
5 cascade : 2 2
do dem prepare 
do actual distribution 
Output file already exists (try and remove): test.tif
get average flow heights 
do dem prepare 
add wh av to dem av 1
add wh av to dem av 2
add wh av to dem av 3
add wh av to dem av 4
add wh av to dem av 5
diffusive max wave cascade: 4 60
5 4 5 4 5 4
replace data 4
done: 4
diffusive max wave cascade: 3 120
14 11 14 11 14 11
replace data 3
done: 3
diffusive max wave cascade: 2 120
40 32 40 32 40 32
replace data 2
done: 2
diffusive max wave cascade: 1 120
118 95 118 95 118 95
replace data 1
done: 1
delete layers 
del1 
del1 
del1 
del1 
del1 
del1 
del1 
 i 00x5faaf8cea090
 i 10x5faaf8d9db00
 i 20x5faaf8cecd10
 i 30x5faaf8d235a0
 i 40x5faaf8d25d00
 i 50x5faaf8d20e10
del1 
del1 
del1 
del1 
copy results 
delete results 
done
do vel output 
End of fastflood function 
Done, writing output
write to:  /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/H.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/Q.tif
Output file already exists (try and remove): /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Tmp/V.tif
Maximum observed q: 1292
Data successfully exported to /app/outputs/fastflood/1000_34_2026-1-19/WI_15/out/06-FLOOD/Discharge/TS_Q_NbS_TR-2.csv
duration: 0.950987 s
done, closing
# ---------------------------------------------------------------------------------------------------
# Estimate of expected annual damage for each scenario 
# ---------------------------------------------------------------------------------------------------
Read Dagame Curve - Ok 
# ---------------------------------------------------------------------------------------------------
# Read Flood Depth - Scenario Current
# ---------------------------------------------------------------------------------------------------
Read flood depth for the Current scenario for Residential damages category- Ok 
Damage estimation for each return period of the Current scenario Residential - Ok 
Estimated annual expected damages for the Current scenario for Residential damages category- Ok- Ok 
Estimated cumulative annual expected damages for the Current scenario for Residential damages category- Ok- Ok 
Read flood depth for the Current scenario for Commercial damages category- Ok 
Damage estimation for each return period of the Current scenario Commercial - Ok 
Estimated annual expected damages for the Current scenario for Commercial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the Current scenario for Commercial damages category- Ok- Ok 
Read flood depth for the Current scenario for Industrial damages category- Ok 
Damage estimation for each return period of the Current scenario Industrial - Ok 
Estimated annual expected damages for the Current scenario for Industrial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the Current scenario for Industrial damages category- Ok- Ok 
Read flood depth for the Current scenario for InfraRoads damages category- Ok 
Damage estimation for each return period of the Current scenario InfraRoads - Ok 
Estimated annual expected damages for the Current scenario for InfraRoads damages category- Ok- Ok 
Estimated cumulative annual expected damages for the Current scenario for InfraRoads damages category- Ok- Ok 
Read flood depth for the Current scenario for Agriculture damages category- Ok 
Damage estimation for each return period of the Current scenario Agriculture - Ok 
Estimated annual expected damages for the Current scenario for Agriculture damages category- Ok- Ok 
Estimated cumulative annual expected damages for the Current scenario for Agriculture damages category- Ok- Ok 
Read flood depth for the BaU scenario for Residential damages category- Ok 
Damage estimation for each return period of the BaU scenario Residential - Ok 
Estimated annual expected damages for the BaU scenario for Residential damages category- Ok- Ok 
Estimated cumulative annual expected damages for the BaU scenario for Residential damages category- Ok- Ok 
Read flood depth for the BaU scenario for Commercial damages category- Ok 
Damage estimation for each return period of the BaU scenario Commercial - Ok 
Estimated annual expected damages for the BaU scenario for Commercial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the BaU scenario for Commercial damages category- Ok- Ok 
Read flood depth for the BaU scenario for Industrial damages category- Ok 
Damage estimation for each return period of the BaU scenario Industrial - Ok 
Estimated annual expected damages for the BaU scenario for Industrial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the BaU scenario for Industrial damages category- Ok- Ok 
Read flood depth for the BaU scenario for InfraRoads damages category- Ok 
Damage estimation for each return period of the BaU scenario InfraRoads - Ok 
Estimated annual expected damages for the BaU scenario for InfraRoads damages category- Ok- Ok 
Estimated cumulative annual expected damages for the BaU scenario for InfraRoads damages category- Ok- Ok 
Read flood depth for the BaU scenario for Agriculture damages category- Ok 
Damage estimation for each return period of the BaU scenario Agriculture - Ok 
Estimated annual expected damages for the BaU scenario for Agriculture damages category- Ok- Ok 
Estimated cumulative annual expected damages for the BaU scenario for Agriculture damages category- Ok- Ok 
Read flood depth for the NbS scenario for Residential damages category- Ok 
Damage estimation for each return period of the NbS scenario Residential - Ok 
Estimated annual expected damages for the NbS scenario for Residential damages category- Ok- Ok 
Estimated cumulative annual expected damages for the NbS scenario for Residential damages category- Ok- Ok 
Read flood depth for the NbS scenario for Commercial damages category- Ok 
Damage estimation for each return period of the NbS scenario Commercial - Ok 
Estimated annual expected damages for the NbS scenario for Commercial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the NbS scenario for Commercial damages category- Ok- Ok 
Read flood depth for the NbS scenario for Industrial damages category- Ok 
Damage estimation for each return period of the NbS scenario Industrial - Ok 
Estimated annual expected damages for the NbS scenario for Industrial damages category- Ok- Ok 
Estimated cumulative annual expected damages for the NbS scenario for Industrial damages category- Ok- Ok 
Read flood depth for the NbS scenario for InfraRoads damages category- Ok 
Damage estimation for each return period of the NbS scenario InfraRoads - Ok 
Estimated annual expected damages for the NbS scenario for InfraRoads damages category- Ok- Ok 
Estimated cumulative annual expected damages for the NbS scenario for InfraRoads damages category- Ok- Ok 
Read flood depth for the NbS scenario for Agriculture damages category- Ok 
Damage estimation for each return period of the NbS scenario Agriculture - Ok 
Estimated annual expected damages for the NbS scenario for Agriculture damages category- Ok- Ok 
Estimated cumulative annual expected damages for the NbS scenario for Agriculture damages category- Ok- Ok 
Correct reading - Scenario Current 
Disaggregation of the scenarios carried out correctly.
ROI.
Indicators.
